[Smart]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
06=Read Channel Margin
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
0D=Soft Read Error Rate stab
B7=SATA Downshift Error Count
B8=End-to-End Error
B9=Head Stability
BA=nduced Op-Vibration Detection
BB=Reported Uncorrectable Errors
BC=Command Timeout
BD=High Fly Writes
BE=Airflow Temperature
BF=G-Sense Error Rate
C0=Power-off Retract Count
C1=Load/Unload Cycle Count
C2=Temperature
C3=Hardware ECC recovered
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
C7=UltraDMA CRC Error Count
C8=Write Error Rate
C9=Soft Read Error Rate
CA=Data Address Mark Error
CB=Run Out Cancel
CC=Soft ECC Correction
CD=Thermal Asperity Rate
CE=Flying Height
CF=Spin High Current
D0=Spin Buzz
D1=Offline Seek Performance
D3=Vibration During Write
D4=Shock During Write
DC=Disk Shift
DD=G-Sense Error Rate
DE=Loaded Hours
DF=Load/Unload Retry Count
E0=Load Friction
E1=Load/Unload Cycle Count
E2=Load 'In'-time
E3=Torque Amplification Count
E4=Power-Off Retract Cycle
E6=GMR Head Amplitude
E7=Temperature
E8=Endurance Remaining
E9=Media Wareout Indicator
F0=Head Flying Hours
F1=Total Host Writes
F2=Total Host Reads
FA=Read Error Retry Rate
FE=Free Fall Protection

[SmartSSD]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
06=Read Channel Margin
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
0D=Soft Read Error Rate stab
C0=Unsafe Shutdown Count
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
F1=Total Host Writes
F2=Total Host Reads
FF=Remaining Life

[SmartIndlinx]
01=Read Error Rate
09=Power-On Hours
0C=Power Cycle Count
B8=Initial Bad Block Count
C2=Temperature
C3=Program Failure Block Count
C4=Erase Failure Block Count
C5=Read Failure Block Count
C6=Total Count of Read Sectors
C7=Total Count of Write Sectors
C8=Total Count of Read Commands
C9=Total Count of Write Commands
CA=Total Count of Error bits from flash
CB=Total Count of Read Sectors with Correctable Bit Errors
CC=Bad Block Full Flag
CD=Maximum PE Count Specification
CE=Minimum Erase Count
CF=Maximum Erase Count
D0=Average Erase Count
D1=Remaining Drive Life

[SmartJMicron60x]
09=Power-On Hours
0C=Power Cycle Count
C2=Temperature
E5=Halt System ID, Flash ID
E8=Firmware Version Information
E9=ECC Fail Record
EA=Average Erase Count, Max Erase Count
EB=Good Block Count, System Block Count

[SmartIntel]
03=Spin Up Time
04=Start/Stop Count
05=Re-Allocated Sector Count
09=Power-On Hours Count
0C=Power Cycle Count
C0=Unsafe Shutdown Count
E1=Host Writes
E8=Available Reserved Space
E9=Media Wearout Indicator
B8=End to End Error Detection Count
AA=Available Reserved Space
AB=Program Fail Count
AC=Erase Fail Count
BB=Uncorrectable Error Count
AE=Unexpected Power Loss
E2=Timed Workload Media Wear
E3=Timed Workload Host Read/Write Ratio
E4=Timed Workload Timer
F1=Total LBAs Written
F2=Total LBAs Read
F9=Total NAND Writes
B7=SATA Downshift Count
BE=Temperature
C7=CRC Error Count
AF=Power Loss Protection Failure
C2=Temperature
C5=Pending Sector Count
EA=Thermal Throttle Status

[SmartSamsung]
05=Reallocated Sector Count
09=Power-on Hours
0C=Power-on Count
AA=Unused Reserved Block Count (Chip) 
AB=Program Fail Count (Chip)
AC=Erase Fail Count (Chip)
AD=Wear Leveling Count
AE=Unexpected Power Loss Count
AF=Program Fail Count (Chip)
B8=Error Detection
E9=Normalized Media Wear-out
B0=Erase Fail Count (Chip)
B1=Wear Leveling Count
B2=Used Reserved Block Count (Chip)
B3=Used Reserved Block Count (Total)
B4=Unused Reserved Block Count (Total)
B5=Program Fail Count (Total)
B6=Erase Fail Count (Total)
B7=Runtime Bad Block (Total)
BB=Uncorrectable Error Count
BE=Airflow Temperature
C2=Temperature
C3=ECC Error Rate
C6=Off-Line Uncorrectable Error Count
C7=CRC Error Count
C9=Super cap Status
CA=SSD Mode Status
EB=POR Recovery Count
F1=Total LBAs Written
F2=Total LBAs Read

[SmartSandForce]
01=Raw Read Error Rate
05=Retired Block Count
09=Power-on Hours
0C=Power Cycle Count
0D=Soft Read Error Rate
64=Gigabytes Erased
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
B1=Wear Range Delta
B5=Program Fail Count
B6=Erase Fail Count
B8=Reported I/O Error Detection Code Errors
BB=Reported Uncorrectable Errors
C2=Temperature
C3=On-the-Fly ECC Uncorrectable Error Count
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
C7=SATA R-Errors (CRC) Error Count
C9=Uncorrectable Soft Read Error Rate
CC=Soft ECC Correction Rate
E6=Life Curve Status
E7=SSD Life Left
E8=Available Reserved Space
EB=SuperCap health
F1=Lifetime Writes from Host
F2=Lifetime Reads from Host

[SmartJMicron61x]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AF=Bad Cluster Table Count (ECC Fail Count)
C0=Unexpected Power Loss Count
C2=Temperature
C5=Current Pending Sector Count
AA=Bad Block Count
AD=Erase Count

[SmartMicron]
01=Raw Read Error Rate
05=Reallocated NAND Blocks
09=Power On Hours
0C=Power Cycle Count
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block-Erase Count
AE=Unexpected Power Loss Count
B4=Unused Reserve NAND Blocks
B5=Unaligned Access Count
B7=SATA Interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
BD=Factory Bad Block Count
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F2=Write Protect Progress
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count

[SmartMicronMU02]
01=Raw Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
0D=Soft Error Rate
0E=Device Capacity (NAND)
0F=User Capacity
10=Spare Blocks Available
11=Remaining Spare Blocks
64=Total Erase Count
AA=Reserved Block Count
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Block-Erase Count
AE=Unexpected Power Loss Count
B4=Unused Reserve NAND Blocks
B7=SATA Interface Downshift
B8=Error Correction Count
BB=Reported Uncorrectable Errors
BC=Command Timeout Count
BD=Factory Bad Block Count
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Smart Off-line Scan Uncorrectable Error Count
C7=Ultra DMA CRC Error Rate
CA=Percent Lifetime Used
CE=Write Error Rate
D2=Successful RAIN Recovery Count
EA=Total Bytes Read
F3=ECC Bits Corrected
F4=ECC Cumulative Threshold Events
F5=Cumulative Program NAND Pages
F6=Total Host Sector Writes
F7=Host Program Page Count
F8=Background Program Page Count
A0=Uncorrectable Sector Count
A1=Valid Spare Blocks
A3=Initial Invalid Blocks
94=Total SLC Erase Count
95=Maximum SLC Erase Count
96=Minimum SLC Erase Count
97=Average SLC Erase Count
A4=Total TLC Erase Count
A5=Maximum TLC Erase Count
A6=Minimum TLC Erase Count
A7=Average TLC Erase Count
A9=Percentage Lifetime Remaining
B5=Program Fail Count
B6=Erase Fail Count
C0=Power-off Retract Count
E8=Available Reserved Space
F1=Total LBA Write
F2=Total LBA Read
F5=Total TLC Write Count
F6=Total SLC Write Count
F7=RAID Recovery Count

[SmartOcz]
01=Raw Read Error Rate
03=Spin Up Time
04=Start Stop Count
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
C2=Temperature
E8=Total Count of Write Sectors
E9=Remaining Life
64=Total Blocks Erased
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Bad Block Count
AD=Erase Count
B8=Factory Bad Block Count
C0=Unexpected Power Loss Count
CA=Total Number of Corrected Bits
CD=Max Rated PE Counts
CE=Minimum Erase Counts
CF=Maximum Erase Counts
D3=SATA Uncorrectable Error Count
D4=NAND Page Reads During Retry
D5=Simple Read Retry Attempts
D6=Adaptive Read Retry Attempts
DD=Internal Data Path Uncorrectable Errors
DE=RAID Recovery Count
E6=Power Loss Protection
FB=NAND Read Count
F1=Total Host Writes
F2=Total Host Reads

[SmartPlextor]
01=Read Error Rate
05=Reallocated Sectors Count
09=Power-On Hours
0C=Power Cycle Count
C0=Unsafe Shutdown Count
C2=Temperature
C4=Reallocation Event Count
C6=Uncorrectable Sector Count
F1=Total LBA written
F2=Total LBA read
B1=Wear Leveling Count
B2=Used Reserved Block Count (Worst Case)
B5=Program Fail Count (Total)
B6=Erase Fail Count (Total)
BB=Uncorrectable Error Count
C7=CRC Error Count
E8=Available Reserved Space
AA=Grown Bad Blocks
AB=Program Fail Count (Total)
AC=Erase Fail Count (Total)
AD=Average Program/Erase Count (Total)
AE=Unexpected Power Loss Count
AF=Program Fail Count (Worst Case)
B0=Erase Fail Count (Worst Case)
B3=Used Reserved Block Count (Total)
B4=UnUsed Reserved Block Count (Total)
B7=SATA Interface Down Shift
B8=End-to-End Data Errors Corrected
BC=Command Time out
C3=ECC rate
E9=NAND GB written

[SmartSanDisk]
05=Retired Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AB=Program Fail Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
C2=Temperature
E8=Remaining Life
F1=Total Host Writes
F2=Total Host Reads

[SmartOczVector]
05=Accumulated Runtime Bad Blocks
09=Power-On Hours Count
0C=Power Cycle Count
AB=Available Over-Provisioned Block Count
AE=Power Cycle Count (Unplanned)
BB=Total Uncorrectable NAND Reads
C2=Temperature
C3=Total Programming Failures
C4=Total Erase Failures
C5=Total Read Failures (Uncorrectable)
C6=Host Reads
C7=Host Writes
D0=Average Erase Count
D2=SATA CRC Error Count
E9=Remaining Life
F9=Total NAND Programming Count
F1=Total Host Writes
F2=Total Host Reads
64=Total Blocks Erased
B8=Factory Bad Block Count Total
CA=Total Number Of Read Bits Corrected
CD=Max Rated PE Count
CE=Min Erase Count
CF=Max Erase Count
D4=Total Count NAND Pages Reads Requiring Read Retry
D5=Total Count of Simple Read Retry Attempts
D6=Total Count of Adaptive Read Retry Attempts
DD=Internal Data Path Protection Uncorrectable Errors
DE=RAID Recovery Count
E0=In Warranty
E1=DAS Polarity
E2=Partial Pfail
E6=Write Throttling Activation Flag
F9=Total NAND Programming Count (pages)
FB=Total NAND Read Count

[SmartCorsair]
01=Raw Read Error Rate
05=Retired Block Count
09=Power On Hours
0C=Power Cycle Count
AA=Reserve Block Count
AC=Erase Fail Count
AE=Unexpected Power Loss Count
B5=Program Fail Count
BB=Reported Uncorrectable Errors
C2=Temperature
C4=Reallocation Event Count
E7=SSD Life Left
F1=Lifetime GB Written
F2=Lifetime GB Read

[SmartToshiba]
01=Read Error Rate
02=Throughput Performance
03=Spin-Up Time
04=Start/Stop Count
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0B=Recalibration Retries
0C=Power Cycle Count
A7=SSD Protect Mode
A8=SATA PHY Error Count
A9=Total Bad Block Count
AD=Erase Count
C0=Unexpected Power Loss Count
C2=Temperature
C4=Reallocation Event Count
C5=Current Pending Sector Count
C6=Uncorrectable Sector Count
F1=Total Host Writes
F2=Total Host Reads

[SmartSanDiskGb]
05=Reallocated Block Count
09=Power On Hours
0C=Power Cycle Count
A6=Min W/E Cycle
A7=Max Bad Block/Die
A8=Maximum Erase Cycle
A9=Total Bad Block
AB=Program Fail Count
AC=Erase Fail Count
AD=Average Erase Cycle
AE=Unexpected Power Loss Count
BB=Reported Uncorrectable Errors
C2=Temperature
D4=SATA PHY Error
E6=Percentage Total P/E Count
E8=Spare Block Remaining
E9=Total GB Written To NAND
F1=Total GB Written
F2=Total GB Read

[SmartMtron]
BB=Total Erase Count

[SmartKingston]
01=Read Error Rate
02=Throughput Performance
03=Spin Up Time
05=Reallocated Sectors Count
07=Seek Error Rate
08=Seek Time Performance
09=Power-On Hours
0A=Spin Retry Count
0C=Power Cycle Count
A8=SATA PHY Error Count
AA=Bad Block Count
AD=Erase count
AF=Bad Cluster Table Count
BB=Uncorrectable Errors
C0=Unsafe Shutdown Count
C2=Temperature
C4=Later Bad Block Count
C5=Current Pending Sector Count
C7=CRC Error Count
DA=CRC Error Count
E7=SSD Life Left
E9=Lifetime Writes to Flash
F0=Write Head
F1=Host Writes
F2=Host Reads
F4=Average Erase Count
F5=Max Erase Count
F6=Total Erase Count

[SmartLongsys]
05=Number of New Bad Block
09=Power-On Hours
0C=Power Cycle Count
A4=Total Erase Count
A5=Max Erase Count
A6=Min Erase Count
A7=Average Erase Count
C0=Power off Retract Cycle
C2=Temperature
C7=Sata CRC Error
F1=Total Written(GB)
F2=Total Read(GB)

[SmartLongsysXT]
01=Read Error Rate
05=Reallocated Sectors Count
09=Power On Hours
0C=Power Cycle Count
A0=Uncorrectable Sector Count on Line
A1=Num Pure Spare
A4=Total Erase Count
A5=Max Erase Count
A6=Min Erase Count
A7=Avg Erase Count
C0=Power Off Retract Count
C2=Temperature	
C3=Hardware ECC recovered
C4=Reallocation Event Count
C6=Uncorrectable Sector Count Off Line
C7=UDMA CRC Error
EF=Fw Update Count
F1=Write Sector Count
F2=Read Sector Count
F3=Backup Block Count
F4=Erase Error Event Count
FA=Low Voltage Count
FB=Static Wear Leveling Count
FC=Data Refresh Count
FD=CODE Refresh Count
FE=WAI

[SmartSMI]
01=Read Error Rate
05=Number of New Bad Block
09=Power-On Hours
0C=Power Cycle Count
A0=Uncorrectable Sector Count On Line
A1=Number of Pure Spare
A3=Number of Initial Invalid Block
A4=Total Erase Count
A5=Max Erase Count
A6=Min Erase Count
A7=Average Erase Count
A8=P/E Cycle
A9=Remain Life Percentage
94=Total Erase Count of SLC
95=Max Erase Count of SLC
96=Min Erase Count of SLC
97=Average Erase Count of SLC
B1=Wear Leveling Count
B5=Program Fail Count
B6=Erase Fail Count
BB=Uncorrectale Error Count
C0=Power off Retract Cycle
C2=Temperature
C3=Cumulative ECC Bit Correction Count
C4=Reallocation Event Count
C5=Current Pending Sector Count
C7=UDMA CRC Error
E8=Available Reserved Space
F1=Total LBAs Written(Unit:32MB)
F2=Total LBAs Read(Unit:32MB)
F5=Total Flash Written(Unit:32M)

[SmartPhison]
01=Number of ECC error
09=Power on hours
0C=Power on/off cycle
A8=SATA PHY error count
AA=Total early/later bad block
AD=Max/Avg erase count
C0=Unexpected power loss count
C2=Temperature
DA=CRC error count
E7=SSD life left
F1=Host Write(GB)

[SmartNVMe]
01=Critical Warning
02=Composite Temperature
03=Available Spare
04=Available Spare Threshold
05=Percentage Used
06=Data Units Read
07=Data Units Written
08=Host Read Commands
09=Host Write Commands
0A=Controller Busy Time
0B=Power Cycles
0C=Power On Hours
0D=Unsafe Shutdowns
0E=Media and Data Integrity Errors
0F=Number of error information log entries